RestoreWinCE on the Roadmate 1200
Hi, 

Ok, let try another way ...

I used files from "Magellan_RoadMate_1200_1215_2_03.exe"
1). Extract all files.
2). Take from folder 'COPY_GROUP_1" file WINCEIMG.BIN ( lenght 5979759 

bytes, from 2007-12-14 17:18:48)
3). Take CLEAN !!! SDMMC Card.
4). Copy WINCEIMG.BIN to root folder of SDMMC Card
5). Make on your PC a text file named WINCEIMG.CKS. Contens of this file 

is:

binsize : 5979759
checksum: 0x24DB1E5F

6). Copy file WINCEIMG.CKS to root folder of SDMMC Card

Now you should restore operationg system from SDMMC Card. 
To do this:
1). Push Power and reset button, go to the Bootloader menu
2). Choice 'Update OS (HDD Format)' option by pushing 'Reset' button
3). Push 'Power' button to confirm operation and bide until message 

'Please remove SD Card !' appear 
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4). Remove SD Card from RoadMate and reset

Now your RoadMate starts with 'clean' WinCE 5.0 Core and you should see 

SysView on the screen.
Follow my previously instrucion to restore the rest of files 

Good luck [image: image2.png]
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Memory Recovery

Hi,

I had a problem with Magellan RoadMate 1200. I had this navigation with empty memory, when its start show me SysView. 
I try to debug file WINCEIMG.BIN and ........ found solution !

It's very simple. I used a SD-CardReader in my PC. Ok, lets run ...

1). Format or clean SDMMC Card (min 64MB)
2). Make in root folder of SDMMC Card file 'GC333AutoRun.inf'. Contens of this file is:

open=\APP\mgnShell.exe

3). Make in root folder of SDMMC Card folder named 'APP'
4). Copy to this folder all files from the backup file of memory (I have this file)
5). Insert SDMMC Card into RoadMate
6). Turn on RoadMate and reset

RoadMate starts with WinCE, then starts file 'mgnShell.exe' from 'APP' folder of SDMMC Card.
'mgnShell.exe' file is a main module of communication subsystem.
Now you can connect USB cable to RoadMate and to your PC. RoadMate is working as USB Storage ! [image: image3.png]



In Windows XP 'My Computer' environment RoadMate's memory is shown as two removable discs: 
- first is TFAT or TFAT32 labeled
- second is without label
Use Copy/Paste method to copy all necessary files to RoadMate.

Good luck for everyone ! [image: image4.png]
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